table_ngc4006_HP9_2025-04.txt Tue Feb 27 17:50:35 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       psl     948.5730    1001.3200    1022.3800      hPa    mean sea level pressure
       prw       0.1292      20.1601      47.6527    kg/m2    vertically integrated water vapor
     cllvi       0.0000      71.2860     738.4120     g/m2    vertically integrated cloud water
     clivi       0.0000      10.4397      81.7417     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0140       0.7060    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0142       0.4434    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0555       0.5984    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.2359     115.3320     mm/d    total precipitation
      prls       0.0000       0.3042      49.3081     mm/d    precip large scale snow
      rsdt       0.0000     338.2290     439.4220     W/m2    top incoming SW radiation(down)
      rsds       0.0000     195.0730     350.4620     W/m2    SW surface(down)
      rsus       0.0000      27.0709     275.1380     W/m2    SW surface(up)
      rsut       0.0000      95.3148     271.1950     W/m2    TOA Outgoing SW Radiation(up)
      rsnt       0.0000     242.9140     392.0630     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       0.0000     168.0020     316.2730     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      67.7793     336.3820     430.8010     W/m2    LW down surface(down)
      rlus      96.5790     397.0470     522.7610     W/m2    LW up surface(up)
      rlus      96.5790     397.0470     522.7610     W/m2    olr(up)
      rlns       1.2468      60.6651     149.7110     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -189.3740       3.6604     153.3760     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -345.8370    -229.0460      14.4756     W/m2    rsns-rlns(down)
        ts     -70.0764      15.0695      36.6748        C    surface temperature
       sic       0.0000       2.7636      99.9996        %    ice cover (fraction of grid box)
       sit       0.0000       0.0451       9.4835        m    ice thickness
       tas     -64.2572      13.9532      35.8205        C    2 m temperature
       uas     -14.9510       0.0516      14.6797      m/s    zonal wind in 10m
       vas     -11.4973      -0.0691      16.1004      m/s    meridional wind in 10m
   sfcwind       0.9864       7.0194      17.9118      m/s    10m Wind Speed
      hfss    -141.0840     -15.1195     141.9980     W/m2    sensible heat flux
      hfls    -280.9000     -87.4830      31.2764     W/m2    latent heat flux
      tauu   -1822.4399      15.0475    3272.3799    mN/m2    u-stress
      tauv   -1879.7500       1.0685    1436.8199    mN/m2    v-stress
      rlus      96.5790     397.0470     522.7610     W/m2    LW up surface
  net_flux    -280.8410       4.7341     349.7450     W/m2    surface net energy flux
      rlnt    -323.7140    -239.2540    -107.6180     W/m2    net top LW radiation  (-OLR)
      rsdt       0.0000     338.2290     439.4220     W/m2    top incoming SW radiation