table_ngc4007_HP9_2020-02.txt Wed Feb 28 06:59:14 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       psl     962.0240    1001.6600    1031.5300      hPa    mean sea level pressure
       prw       0.2967      21.4163      55.4952    kg/m2    vertically integrated water vapor
     cllvi       0.0000      88.8445     975.6930     g/m2    vertically integrated cloud water
     clivi       0.0000      10.0748      93.7856     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0124       0.8929    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0151       0.6392    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0540       1.2268    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.3153     205.8130     mm/d    total precipitation
      prls       0.0000       0.3177      93.0637     mm/d    precip large scale snow
      rsdt       0.0000     348.7880     461.5500     W/m2    top incoming SW radiation(down)
      rsds       0.0000     194.2570     376.5550     W/m2    SW surface(down)
      rsus       0.0000      26.1692     249.5660     W/m2    SW surface(up)
      rsut       0.0000     102.7110     292.6420     W/m2    TOA Outgoing SW Radiation(up)
      rsnt       0.0000     246.0770     402.3730     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       0.0000     168.0880     319.6600     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      94.5995     336.9380     438.9080     W/m2    LW down surface(down)
      rlus     141.5320     391.9750     573.5740     W/m2    LW up surface(up)
      rlus     141.5320     391.9750     573.5740     W/m2    olr(up)
      rlns     -14.1480      55.0363     147.9250     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -199.0490       6.2800     165.9600     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -356.6690    -223.8870     -21.9947     W/m2    rsns-rlns(down)
        ts     -49.7246      13.8248      43.1299        C    surface temperature
       sic       0.0000       2.7405     100.0000        %    ice cover (fraction of grid box)
       sit       0.0000       0.0404      10.2693        m    ice thickness
       tas     -44.3348      12.4976      33.3539        C    2 m temperature
       uas     -13.6239      -0.3965      21.6866      m/s    zonal wind in 10m
       vas     -16.1787      -0.5116      13.7371      m/s    meridional wind in 10m
   sfcwind       0.8819       6.9899      24.1613      m/s    10m Wind Speed
      hfss    -239.8420     -15.0033     853.0970     W/m2    sensible heat flux
      hfls    -412.6970     -89.6130     196.2290     W/m2    latent heat flux
      tauu   -2809.9099       9.7742    5400.9502    mN/m2    u-stress
      tauv   -3137.5801      -7.2670    2333.9900    mN/m2    v-stress
      rlus     141.5320     391.9750     573.5740     W/m2    LW up surface
  net_flux    -598.5550       8.4353     782.1930     W/m2    surface net energy flux
      rlnt    -314.4320    -239.7970    -134.3820     W/m2    net top LW radiation  (-OLR)
      rsdt       0.0000     348.7880     461.5500     W/m2    top incoming SW radiation