table_ngc4007_HP9_2020-03.txt Tue Feb 20 11:23:20 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       prw       0.2116      21.5070      54.1908    kg/m2    vertically integrated water vapor
     cllvi       0.0000      84.7799    1011.7200     g/m2    vertically integrated cloud water
     clivi       0.0000      10.7298      80.5904     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0136       0.7539    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0149       0.5110    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0526       1.0488    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.3054     147.1520     mm/d    total precipitation
      prls       0.0000       0.3195      81.1062     mm/d    precip large scale snow
      rsdt      17.7702     343.8230     437.3790     W/m2    top incoming SW radiation(down)
      rsds       7.4593     194.2860     353.2170     W/m2    SW surface(down)
      rsus       2.1047      26.0598     262.1090     W/m2    SW surface(up)
      rsut      10.7865      98.7667     275.0160     W/m2    TOA Outgoing SW Radiation(up)
      rsnt       6.9382     245.0560     388.4690     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       1.4536     168.2260     304.2240     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      73.6848     339.9860     442.7530     W/m2    LW down surface(down)
      rlus     112.5590     395.6220     547.3020     W/m2    LW up surface(up)
      rlus     112.5590     395.6220     547.3020     W/m2    olr(up)
      rlns      -4.5908      55.6361     163.5170     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -162.0730       6.2191     162.3740     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -350.1660    -227.3960      -9.2039     W/m2    rsns-rlns(down)
        ts     -62.1739      14.5307      39.5207        C    surface temperature
       sic       0.0000       2.7440     100.0000        %    ice cover (fraction of grid box)
       sit       0.0000       0.0474      10.5668        m    ice thickness
       tas     -58.0441      13.1588      35.2460        C    2 m temperature
       uas     -14.5843      -0.3176      18.5983      m/s    zonal wind in 10m
       vas     -13.0078      -0.2852      14.5975      m/s    meridional wind in 10m
   sfcwind       0.7459       6.9662      21.3012      m/s    10m Wind Speed
      hfss    -196.2870     -16.5134     278.3740     W/m2    sensible heat flux
      hfls    -323.5630     -90.0227     123.9850     W/m2    latent heat flux
      tauu   -2043.2000      11.3100    4425.5000    mN/m2    u-stress
      tauv   -2098.8601      -2.1483    1228.7700    mN/m2    v-stress
      rlus     112.5590     395.6220     547.3020     W/m2    LW up surface
  net_flux    -397.2010       6.0538     416.0380     W/m2    surface net energy flux
      rlnt    -315.1150    -238.8370    -123.8740     W/m2    net top LW radiation  (-OLR)
      rsdt      17.7702     343.8230     437.3790     W/m2    top incoming SW radiation