table_ngc4007_2020-04.txt Mon Feb 26 08:08:36 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       psl     950.5830    1001.3500    1018.0500      hPa    mean sea level pressure
       prw       0.1242      21.6945      52.8811    kg/m2    vertically integrated water vapor
     cllvi       0.0000      86.1292     845.2520     g/m2    vertically integrated cloud water
     clivi       0.0000      10.8060      92.2759     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0141       0.7428    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0150       0.4270    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0541       0.8632    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.3264     151.9330     mm/d    total precipitation
      prls       0.0000       0.3155     108.8490     mm/d    precip large scale snow
      rsdt       0.0000     337.9740     439.2430     W/m2    top incoming SW radiation(down)
      rsds       0.0000     191.8020     350.9740     W/m2    SW surface(down)
      rsus       0.0000      26.8293     276.1140     W/m2    SW surface(up)
      rsut       0.0000      96.9098     269.8120     W/m2    TOA Outgoing SW Radiation(up)
      rsnt       0.0000     241.0640     391.3420     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       0.0000     164.9720     315.2000     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      63.6163     344.5490     438.9260     W/m2    LW down surface(down)
      rlus      90.8229     400.1560     556.6240     W/m2    LW up surface(up)
      rlus      90.8229     400.1560     556.6240     W/m2    olr(up)
      rlns      -8.0715      55.6069     165.6490     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -192.9770       1.4529     141.6770     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -354.4430    -235.1840       5.9521     W/m2    rsns-rlns(down)
        ts     -73.1646      15.5442      40.8390        C    surface temperature
       sic       0.0000       2.6720     100.0000        %    ice cover (fraction of grid box)
       sit       0.0000       0.0522      10.6267        m    ice thickness
       tas     -67.4190      14.1806      37.0236        C    2 m temperature
       uas     -14.9711      -0.2645      21.9367      m/s    zonal wind in 10m
       vas     -13.4027      -0.0527      16.6818      m/s    meridional wind in 10m
   sfcwind       0.8470       6.9561      23.9852      m/s    10m Wind Speed
      hfss    -197.9170     -18.2940     343.2440     W/m2    sensible heat flux
      hfls    -350.8110     -90.7171     114.2200     W/m2    latent heat flux
      tauu   -1733.1000      10.9157    4843.7002    mN/m2    u-stress
      tauv   -1984.6500       2.0702    1125.3500    mN/m2    v-stress
      rlus      90.8229     400.1560     556.6240     W/m2    LW up surface
  net_flux    -445.6610       0.3542     360.3770     W/m2    surface net energy flux
      rlnt    -320.6270    -239.6110    -102.7970     W/m2    net top LW radiation  (-OLR)
      rsdt       0.0000     337.9740     439.2430     W/m2    top incoming SW radiation