table_ngc4007_HP9_2020-JJA.txt Tue Feb 27 14:41:37 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       psl     945.5210    1000.9500    1019.7900      hPa    mean sea level pressure
       prw       0.0783      23.8675      64.4560    kg/m2    vertically integrated water vapor
     cllvi       0.0000      98.2882    1279.0800     g/m2    vertically integrated cloud water
     clivi       0.0000       9.6405      85.5266     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0137       0.9509    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0164       0.4072    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0535       0.8466    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.4486     149.8510     mm/d    total precipitation
      prls       0.0000       0.2179      69.8396     mm/d    precip large scale snow
      rsdt       0.0000     330.3140     459.4780     W/m2    top incoming SW radiation(down)
      rsds       0.0000     178.4570     390.4830     W/m2    SW surface(down)
      rsus       0.0000      22.3416     307.3540     W/m2    SW surface(up)
      rsut       0.0000      95.9392     292.9520     W/m2    TOA Outgoing SW Radiation(up)
      rsnt       0.0000     234.3740     408.0710     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       0.0000     156.1160     328.1750     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      55.4136     353.4250     465.2270     W/m2    LW down surface(down)
      rlus      83.5028     407.2740     569.8400     W/m2    LW up surface(up)
      rlus      83.5028     407.2740     569.8400     W/m2    olr(up)
      rlns     -16.6438      53.8489     169.7400     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -183.9880      -9.5864     151.3450     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -386.6090    -251.1580     -30.2686     W/m2    rsns-rlns(down)
        ts     -77.5135      16.8807      43.3129        C    surface temperature
       sic       0.0000       3.8404      99.9887        %    ice cover (fraction of grid box)
       sit       0.0000       0.0403       7.7398        m    ice thickness
       tas     -70.9760      15.6635      41.7389        C    2 m temperature
       uas     -13.2019       0.1639      16.2280      m/s    zonal wind in 10m
       vas     -13.3051       0.7031      16.1950      m/s    meridional wind in 10m
   sfcwind       0.7855       7.3303      19.8046      m/s    10m Wind Speed
      hfss    -198.1260     -19.0937     253.2680     W/m2    sensible heat flux
      hfls    -354.8740     -94.1180     144.1020     W/m2    latent heat flux
      tauu   -1908.9600      18.1404    3580.8401    mN/m2    u-stress
      tauv   -1625.1100       7.2598    2326.8601    mN/m2    v-stress
      rlus      83.5028     407.2740     569.8400     W/m2    LW up surface
  net_flux    -410.7670     -10.9448     363.1090     W/m2    surface net energy flux
      rlnt    -341.0350    -243.9610     -90.3418     W/m2    net top LW radiation  (-OLR)
      rsdt       0.0000     330.3140     459.4780     W/m2    top incoming SW radiation