table_ngc4007_HP9_2020-MAM.txt Tue Feb 27 14:21:33 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       psl     954.3690    1001.3400    1019.2600      hPa    mean sea level pressure
       prw       0.1535      21.7766      52.0612    kg/m2    vertically integrated water vapor
     cllvi       0.0000      86.9923     858.1660     g/m2    vertically integrated cloud water
     clivi       0.0054      10.7270      76.7617     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0139       0.6351    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0151       0.3615    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0541       0.6073    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.3412     132.8200     mm/d    total precipitation
      prls       0.0000       0.2940      87.1627     mm/d    precip large scale snow
      rsdt      20.9124     338.2300     433.3140     W/m2    top incoming SW radiation(down)
      rsds      10.1592     190.6210     336.6180     W/m2    SW surface(down)
      rsus       1.2763      26.3322     265.9100     W/m2    SW surface(up)
      rsut      12.5421      97.5682     265.5830     W/m2    TOA Outgoing SW Radiation(up)
      rsnt       6.3238     240.6620     384.6650     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       2.0377     164.2890     301.3360     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      67.6904     344.3650     438.5190     W/m2    LW down surface(down)
      rlus      96.8040     399.7860     549.3300     W/m2    LW up surface(up)
      rlus      96.8040     399.7860     549.3300     W/m2    olr(up)
      rlns      -2.7559      55.4211     153.7800     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -176.1290       0.9587     132.4490     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -344.4970    -235.4980       8.8830     W/m2    rsns-rlns(down)
        ts     -70.2390      15.4497      39.8079        C    surface temperature
       sic       0.0000       2.8195      99.9996        %    ice cover (fraction of grid box)
       sit       0.0000       0.0506       9.5658        m    ice thickness
       tas     -64.8744      14.0951      36.1904        C    2 m temperature
       uas     -14.3400      -0.2389      18.5514      m/s    zonal wind in 10m
       vas     -12.7946      -0.0139      15.4191      m/s    meridional wind in 10m
   sfcwind       0.8970       6.9796      21.4010      m/s    10m Wind Speed
      hfss    -192.1270     -18.0812     278.5410     W/m2    sensible heat flux
      hfls    -304.1110     -91.2992      85.9254     W/m2    latent heat flux
      tauu   -1709.4301      11.5386    4234.9199    mN/m2    u-stress
      tauv   -1721.4700       0.8473    1111.9200    mN/m2    v-stress
      rlus      96.8040     399.7860     549.3300     W/m2    LW up surface
  net_flux    -393.2520      -0.5127     322.9580     W/m2    surface net energy flux
      rlnt    -311.2290    -239.7030    -108.0620     W/m2    net top LW radiation  (-OLR)
      rsdt      20.9124     338.2300     433.3140     W/m2    top incoming SW radiation