table_ngc4007_HP9_2020-SON.txt Tue Feb 27 15:08:43 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       psl     944.2560    1001.2500    1020.9800      hPa    mean sea level pressure
       prw       0.1070      21.9159      51.5229    kg/m2    vertically integrated water vapor
     cllvi       0.0000      92.0087    1087.2300     g/m2    vertically integrated cloud water
     clivi       0.0000      10.0864      73.5355     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0132       0.8775    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0153       0.3580    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0535       0.7344    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.3242     132.2900     mm/d    total precipitation
      prls       0.0000       0.2948      70.4469     mm/d    precip large scale snow
      rsdt      25.0567     342.0660     437.1280     W/m2    top incoming SW radiation(down)
      rsds       6.4385     190.6100     375.9430     W/m2    SW surface(down)
      rsus       0.4833      27.3924     252.3450     W/m2    SW surface(up)
      rsut      10.8883     101.8490     272.3050     W/m2    TOA Outgoing SW Radiation(up)
      rsnt       9.7358     240.2170     383.6540     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       2.6891     163.2180     326.8760     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      62.0418     343.7850     435.7200     W/m2    LW down surface(down)
      rlus     102.9870     398.3960     522.1450     W/m2    LW up surface(up)
      rlus     102.9870     398.3960     522.1450     W/m2    olr(up)
      rlns       4.4595      54.6108     177.8380     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -180.8210      -0.7253     136.1290     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -358.1260    -235.1780      33.4228     W/m2    rsns-rlns(down)
        ts     -68.2194      15.2306      36.3409        C    surface temperature
       sic       0.0000       4.1321      99.9051        %    ice cover (fraction of grid box)
       sit       0.0000       0.0431       9.8749        m    ice thickness
       tas     -63.2995      13.9385      33.1568        C    2 m temperature
       uas     -14.2931      -0.0332      17.3661      m/s    zonal wind in 10m
       vas     -13.3902       0.2645      14.3660      m/s    meridional wind in 10m
   sfcwind       0.9378       7.3019      19.8191      m/s    10m Wind Speed
      hfss    -198.0240     -16.4996     200.8630     W/m2    sensible heat flux
      hfls    -324.9070     -89.1609      79.2690     W/m2    latent heat flux
      tauu   -1480.6899      17.0552    4629.0498    mN/m2    u-stress
      tauv   -2227.2100       1.6346    1503.6200    mN/m2    v-stress
      rlus     102.9870     398.3960     522.1450     W/m2    LW up surface
  net_flux    -265.5180       2.9462     215.4560     W/m2    surface net energy flux
      rlnt    -318.0920    -240.9420    -104.5860     W/m2    net top LW radiation  (-OLR)
      rsdt      25.0567     342.0660     437.1280     W/m2    top incoming SW radiation