table_ngc4008_HP9_2020-02.txt Tue Feb 27 21:52:52 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       psl     963.1420    1001.6500    1028.5699      hPa    mean sea level pressure
       prw       0.2857      21.4617      56.2485    kg/m2    vertically integrated water vapor
     cllvi       0.0000      88.7216     937.0120     g/m2    vertically integrated cloud water
     clivi       0.0000      10.0608     107.8360     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0129       0.7414    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0149       0.4917    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0523       1.6463    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.2991     167.4540     mm/d    total precipitation
      prls       0.0000       0.2993      72.5179     mm/d    precip large scale snow
      rsdt       0.0000     348.8610     462.1950     W/m2    top incoming SW radiation(down)
      rsds       0.0000     194.8560     386.3200     W/m2    SW surface(down)
      rsus       0.0000      26.1535     223.7910     W/m2    SW surface(up)
      rsut       0.0000     102.1740     299.7020     W/m2    TOA Outgoing SW Radiation(up)
      rsnt       0.0000     246.6870     411.1480     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       0.0000     168.7030     329.7220     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      89.3820     337.4100     440.1480     W/m2    LW down surface(down)
      rlus     143.6380     392.0240     556.1460     W/m2    LW up surface(up)
      rlus     143.6380     392.0240     556.1460     W/m2    olr(up)
      rlns     -18.8315      54.6139     156.6240     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -191.9080       7.5834     159.3210     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -365.0200    -223.3220      -8.9051     W/m2    rsns-rlns(down)
        ts     -49.3369      13.8171      40.7259        C    surface temperature
       sic       0.0000       2.6926     100.0000        %    ice cover (fraction of grid box)
       sit       0.0000       0.0410      10.1859        m    ice thickness
       tas     -45.8148      12.4963      34.0849        C    2 m temperature
       uas     -14.2433      -0.3498      17.8554      m/s    zonal wind in 10m
       vas     -15.4838      -0.4628      14.4670      m/s    meridional wind in 10m
   sfcwind       0.9301       7.0389      20.0061      m/s    10m Wind Speed
      hfss    -298.0050     -15.1890     568.7310     W/m2    sensible heat flux
      hfls    -378.6800     -89.3976     249.8800     W/m2    latent heat flux
      tauu   -3097.2300      10.4283    3483.9900    mN/m2    u-stress
      tauv   -3135.5000      -5.7875    2510.8999    mN/m2    v-stress
      rlus     143.6380     392.0240     556.1460     W/m2    LW up surface
  net_flux    -583.9080       9.5021     843.8390     W/m2    surface net energy flux
      rlnt    -313.0070    -239.1040    -141.1720     W/m2    net top LW radiation  (-OLR)
      rsdt       0.0000     348.8610     462.1950     W/m2    top incoming SW radiation