table_ngc4008_HP9_2020-04.txt Tue Feb 27 10:42:44 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       psl     959.0940    1001.3400    1020.1600      hPa    mean sea level pressure
       prw       0.1770      22.1150      53.6810    kg/m2    vertically integrated water vapor
     cllvi       0.0000      87.0220     987.5920     g/m2    vertically integrated cloud water
     clivi       0.0001      10.8823      74.4521     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0142       0.8007    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0152       0.5375    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0551       0.8255    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.3629     162.7270     mm/d    total precipitation
      prls       0.0000       0.3183      77.4740     mm/d    precip large scale snow
      rsdt       0.0000     337.9740     439.2430     W/m2    top incoming SW radiation(down)
      rsds       0.0000     191.1760     346.8310     W/m2    SW surface(down)
      rsus       0.0000      26.7150     275.1990     W/m2    SW surface(up)
      rsut       0.0000      97.1331     270.8490     W/m2    TOA Outgoing SW Radiation(up)
      rsnt       0.0000     240.8410     391.1430     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       0.0000     164.4610     302.5220     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      73.1424     345.2410     443.2980     W/m2    LW down surface(down)
      rlus      95.6209     400.2980     540.5010     W/m2    LW up surface(up)
      rlus      95.6209     400.2980     540.5010     W/m2    olr(up)
      rlns      -4.7657      55.0577     150.9060     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -191.8010       1.5422     140.5710     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -352.3370    -235.8370       7.4128     W/m2    rsns-rlns(down)
        ts     -70.4892      15.5885      39.1433        C    surface temperature
       sic       0.0000       2.6518     100.0000        %    ice cover (fraction of grid box)
       sit       0.0000       0.0525      11.0750        m    ice thickness
       tas     -64.9398      14.2530      36.3874        C    2 m temperature
       uas     -14.4603      -0.2705      18.7673      m/s    zonal wind in 10m
       vas     -13.3676      -0.0024      15.2127      m/s    meridional wind in 10m
   sfcwind       0.9825       7.0558      21.7660      m/s    10m Wind Speed
      hfss    -198.0710     -17.8771     279.0660     W/m2    sensible heat flux
      hfls    -307.0720     -91.4946      73.9250     W/m2    latent heat flux
      tauu   -2034.4700      14.1878    3806.8899    mN/m2    u-stress
      tauv   -2038.7000       2.4184    1075.4900    mN/m2    v-stress
      rlus      95.6209     400.2980     540.5010     W/m2    LW up surface
  net_flux    -403.0770       0.0320     323.5130     W/m2    surface net energy flux
      rlnt    -317.2920    -239.2990    -109.1630     W/m2    net top LW radiation  (-OLR)
      rsdt       0.0000     337.9740     439.2430     W/m2    top incoming SW radiation