table_ngc4008_HP9_2020-JJA.txt Mon Feb 26 09:43:08 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       psl     945.2320    1000.9400    1021.3200      hPa    mean sea level pressure
       prw       0.0816      23.8180      64.8126    kg/m2    vertically integrated water vapor
     cllvi       0.0000      98.1681    1480.5699     g/m2    vertically integrated cloud water
     clivi       0.0000       9.6891     100.7250     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0138       0.9648    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0163       0.3871    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0534       0.9382    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.4436     159.5970     mm/d    total precipitation
      prls       0.0000       0.2168      85.7653     mm/d    precip large scale snow
      rsdt       0.0000     330.2760     460.0340     W/m2    top incoming SW radiation(down)
      rsds       0.0000     179.0130     388.3340     W/m2    SW surface(down)
      rsus       0.0000      22.2935     299.0900     W/m2    SW surface(up)
      rsut       0.0000      95.3332     285.4130     W/m2    TOA Outgoing SW Radiation(up)
      rsnt       0.0000     234.9430     407.9220     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       0.0000     156.7200     323.1280     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      54.7005     353.6480     460.5690     W/m2    LW down surface(down)
      rlus      75.8364     407.6680     578.4420     W/m2    LW up surface(up)
      rlus      75.8364     407.6680     578.4420     W/m2    olr(up)
      rlns     -15.8354      54.0201     179.1840     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -185.5350      -9.0618     150.4820     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -388.2770    -250.9480     -21.7723     W/m2    rsns-rlns(down)
        ts     -81.9666      16.9647      43.6189        C    surface temperature
       sic       0.0000       3.6356      99.9506        %    ice cover (fraction of grid box)
       sit       0.0000       0.0373       7.2914        m    ice thickness
       tas     -74.8590      15.7359      41.5748        C    2 m temperature
       uas     -13.3145       0.1184      18.6379      m/s    zonal wind in 10m
       vas     -13.4404       0.6874      16.3430      m/s    meridional wind in 10m
   sfcwind       0.8030       7.2914      22.0949      m/s    10m Wind Speed
      hfss    -195.1830     -19.1174     303.9470     W/m2    sensible heat flux
      hfls    -342.7910     -93.9937     125.0910     W/m2    latent heat flux
      tauu   -1783.7400      16.8984    4096.6201    mN/m2    u-stress
      tauv   -1835.5800       7.4902    2268.6001    mN/m2    v-stress
      rlus      75.8364     407.6680     578.4420     W/m2    LW up surface
  net_flux    -378.5400     -10.4117     334.8620     W/m2    surface net energy flux
      rlnt    -339.4980    -244.0040     -85.0693     W/m2    net top LW radiation  (-OLR)
      rsdt       0.0000     330.2760     460.0340     W/m2    top incoming SW radiation