table_ngc4008_HP9_2020-MAM.txt Mon Feb 26 09:24:50 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       psl     957.4330    1001.3200    1018.7100      hPa    mean sea level pressure
       prw       0.1904      22.0471      53.1805    kg/m2    vertically integrated water vapor
     cllvi       0.0000      88.0004     849.4180     g/m2    vertically integrated cloud water
     clivi       0.0034      10.5766      69.3214     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0140       0.6293    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0153       0.3873    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0539       0.8144    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.3650     120.0840     mm/d    total precipitation
      prls       0.0000       0.2869      72.4408     mm/d    precip large scale snow
      rsdt      20.9124     338.2300     433.3140     W/m2    top incoming SW radiation(down)
      rsds      12.6325     190.5520     336.5590     W/m2    SW surface(down)
      rsus       1.0773      26.1831     268.8790     W/m2    SW surface(up)
      rsut      13.2200      97.3478     265.0050     W/m2    TOA Outgoing SW Radiation(up)
      rsnt       6.9288     240.8820     382.6150     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       2.5581     164.3690     302.3560     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      73.1131     345.1980     439.8520     W/m2    LW down surface(down)
      rlus     100.7190     400.2150     534.7450     W/m2    LW up surface(up)
      rlus     100.7190     400.2150     534.7450     W/m2    olr(up)
      rlns      -1.0041      55.0171     152.0510     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -171.5310       0.8426     133.8840     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -351.5210    -235.8460       1.5713     W/m2    rsns-rlns(down)
        ts     -68.2196      15.5526      38.2719        C    surface temperature
       sic       0.0000       2.6739      99.9976        %    ice cover (fraction of grid box)
       sit       0.0000       0.0510      10.7545        m    ice thickness
       tas     -62.9729      14.2340      35.8307        C    2 m temperature
       uas     -13.9870      -0.2740      16.3528      m/s    zonal wind in 10m
       vas     -12.0789      -0.0062      14.3048      m/s    meridional wind in 10m
   sfcwind       1.0936       7.0982      19.1711      m/s    10m Wind Speed
      hfss    -192.5240     -18.1030     221.6940     W/m2    sensible heat flux
      hfls    -285.1500     -91.8042      76.9971     W/m2    latent heat flux
      tauu   -1815.7700      11.7340    3460.0500    mN/m2    u-stress
      tauv   -1635.2100       1.2555    1223.4700    mN/m2    v-stress
      rlus     100.7190     400.2150     534.7450     W/m2    LW up surface
  net_flux    -331.2930      -0.5548     299.9910     W/m2    surface net energy flux
      rlnt    -315.5710    -240.0390    -111.7980     W/m2    net top LW radiation  (-OLR)
      rsdt      20.9124     338.2300     433.3140     W/m2    top incoming SW radiation