table_ngc4008_HP9_2020-SON.txt Tue Feb 27 11:09:14 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       psl     946.7090    1001.2600    1022.6800      hPa    mean sea level pressure
       prw       0.1185      21.8515      51.2973    kg/m2    vertically integrated water vapor
     cllvi       0.0000      90.3409    1043.8800     g/m2    vertically integrated cloud water
     clivi       0.0000      10.1024      76.7956     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0133       0.8100    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0152       0.3992    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0536       0.8592    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.3164     146.0200     mm/d    total precipitation
      prls       0.0000       0.2808      72.1280     mm/d    precip large scale snow
      rsdt      25.0567     342.0660     437.1280     W/m2    top incoming SW radiation(down)
      rsds       7.5723     191.3590     380.3920     W/m2    SW surface(down)
      rsus       0.5936      27.3011     248.8720     W/m2    SW surface(up)
      rsut      10.9910     101.0630     267.9720     W/m2    TOA Outgoing SW Radiation(up)
      rsnt      10.7670     241.0030     385.3680     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       3.2516     164.0580     328.8240     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      63.1127     343.8350     433.8500     W/m2    LW down surface(down)
      rlus     100.7610     398.7770     521.5610     W/m2    LW up surface(up)
      rlus     100.7610     398.7770     521.5610     W/m2    olr(up)
      rlns       5.0462      54.9414     181.6480     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -183.7530      -0.1222     133.2950     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -359.1620    -234.7190      42.8735     W/m2    rsns-rlns(down)
        ts     -69.0104      15.3175      36.3722        C    surface temperature
       sic       0.0000       4.0477      99.8676        %    ice cover (fraction of grid box)
       sit       0.0000       0.0402       7.6981        m    ice thickness
       tas     -63.7710      14.0099      33.1938        C    2 m temperature
       uas     -14.4223      -0.1083      18.8387      m/s    zonal wind in 10m
       vas     -12.8339       0.2779      14.9696      m/s    meridional wind in 10m
   sfcwind       0.9285       7.2446      20.9772      m/s    10m Wind Speed
      hfss    -199.1220     -16.7452     212.2590     W/m2    sensible heat flux
      hfls    -305.5680     -88.9817      56.1205     W/m2    latent heat flux
      tauu   -1453.7500      14.8940    4764.8599    mN/m2    u-stress
      tauv   -2057.5000       0.4723    1181.9399    mN/m2    v-stress
      rlus     100.7610     398.7770     521.5610     W/m2    LW up surface
  net_flux    -297.0670       3.3895     214.1500     W/m2    surface net energy flux
      rlnt    -313.0680    -241.1260    -105.1370     W/m2    net top LW radiation  (-OLR)
      rsdt      25.0567     342.0660     437.1280     W/m2    top incoming SW radiation