table_ngc4008_HP9_2025-04.txt Tue Feb 27 11:24:36 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       psl     945.3360    1001.3100    1019.6200      hPa    mean sea level pressure
       prw       0.1094      20.4317      48.7139    kg/m2    vertically integrated water vapor
     cllvi       0.0000      82.2386     822.6550     g/m2    vertically integrated cloud water
     clivi       0.0000      10.4670      86.6499     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0140       0.8510    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0140       0.3889    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0528       0.9338    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.1940     138.8590     mm/d    total precipitation
      prls       0.0000       0.3105      73.5927     mm/d    precip large scale snow
      rsdt       0.0000     338.2290     439.4220     W/m2    top incoming SW radiation(down)
      rsds       0.0000     194.1240     353.8050     W/m2    SW surface(down)
      rsus       0.0000      27.2168     278.1020     W/m2    SW surface(up)
      rsut       0.0000      95.9635     270.4090     W/m2    TOA Outgoing SW Radiation(up)
      rsnt       0.0000     242.2660     391.7880     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       0.0000     166.9070     317.1620     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      63.1022     340.4000     435.5980     W/m2    LW down surface(down)
      rlus      85.9255     397.9130     536.1510     W/m2    LW up surface(up)
      rlus      85.9255     397.9130     536.1510     W/m2    olr(up)
      rlns      -5.8942      57.5129     153.4650     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -188.1690       3.0037     152.0120     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -340.3010    -231.0060      23.0554     W/m2    rsns-rlns(down)
        ts     -75.8459      15.1538      38.5828        C    surface temperature
       sic       0.0000       3.1410      99.9999        %    ice cover (fraction of grid box)
       sit       0.0000       0.0560      10.5606        m    ice thickness
       tas     -69.4213      13.8014      37.3228        C    2 m temperature
       uas     -13.9283      -0.0106      17.9374      m/s    zonal wind in 10m
       vas     -13.1092      -0.0429      15.9789      m/s    meridional wind in 10m
   sfcwind       1.0324       7.0128      20.3287      m/s    10m Wind Speed
      hfss    -200.7630     -19.2435     263.3620     W/m2    sensible heat flux
      hfls    -294.7530     -86.6313      61.9400     W/m2    latent heat flux
      tauu   -1987.5900      16.1191    4945.7300    mN/m2    u-stress
      tauv   -2148.0200      -0.1664    1141.0800    mN/m2    v-stress
      rlus      85.9255     397.9130     536.1510     W/m2    LW up surface
  net_flux    -361.5470       3.5193     329.4950     W/m2    surface net energy flux
      rlnt    -324.0620    -239.2620    -100.0750     W/m2    net top LW radiation  (-OLR)
      rsdt       0.0000     338.2290     439.4220     W/m2    top incoming SW radiation