table_ngc4008_HP9_2025-MAM.txt Tue Feb 27 11:39:22 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       psl     957.9200    1001.3400    1017.6300      hPa    mean sea level pressure
       prw       0.1458      20.5423      47.6428    kg/m2    vertically integrated water vapor
     cllvi       0.0000      82.4678     764.0510     g/m2    vertically integrated cloud water
     clivi       0.0003      10.3704      84.6300     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0141       0.9701    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0142       0.3667    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0531       0.7256    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.2231     121.3700     mm/d    total precipitation
      prls       0.0000       0.2997      75.3001     mm/d    precip large scale snow
      rsdt      21.3696     338.4710     433.4800     W/m2    top incoming SW radiation(down)
      rsds      12.6140     193.6380     339.8520     W/m2    SW surface(down)
      rsus       1.3735      26.6893     270.9140     W/m2    SW surface(up)
      rsut      13.6778      95.9469     264.3280     W/m2    TOA Outgoing SW Radiation(up)
      rsnt       6.8345     242.5240     383.6080     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       2.5114     166.9490     302.9300     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      68.0003     340.1880     428.2520     W/m2    LW down surface(down)
      rlus      92.5106     397.8800     526.8090     W/m2    LW up surface(up)
      rlus      92.5106     397.8800     526.8090     W/m2    olr(up)
      rlns      -2.9185      57.6918     153.2920     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -167.9460       3.1361     139.2910     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -333.9100    -230.9310       8.4642     W/m2    rsns-rlns(down)
        ts     -72.4054      15.1511      37.1683        C    surface temperature
       sic       0.0000       3.1411      99.9977        %    ice cover (fraction of grid box)
       sit       0.0000       0.0542       9.6851        m    ice thickness
       tas     -66.3257      13.7920      35.5531        C    2 m temperature
       uas     -13.6093      -0.0877      16.8404      m/s    zonal wind in 10m
       vas     -12.4252      -0.0450      15.1954      m/s    meridional wind in 10m
   sfcwind       1.1163       6.9794      19.7789      m/s    10m Wind Speed
      hfss    -189.6610     -19.3445     227.8310     W/m2    sensible heat flux
      hfls    -263.6050     -87.8351      37.7700     W/m2    latent heat flux
      tauu   -1781.4301      12.7026    3786.3201    mN/m2    u-stress
      tauv   -1656.1100      -0.4291    1633.0699    mN/m2    v-stress
      rlus      92.5106     397.8800     526.8090     W/m2    LW up surface
  net_flux    -348.3240       2.0775     281.0640     W/m2    surface net energy flux
      rlnt    -322.2450    -239.3880    -105.8980     W/m2    net top LW radiation  (-OLR)
      rsdt      21.3696     338.4710     433.4800     W/m2    top incoming SW radiation