table_ngc4008_HP9_2025-SON.txt Wed Feb 28 07:26:11 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       psl     951.0600    1001.2600    1021.8300      hPa    mean sea level pressure
       prw       0.1148      21.4374      49.4227    kg/m2    vertically integrated water vapor
     cllvi       0.0000      87.3251     796.0020     g/m2    vertically integrated cloud water
     clivi       0.0000       9.9880      98.4252     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0135       0.8036    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0147       0.4018    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0530       0.8353    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.2579     140.4240     mm/d    total precipitation
      prls       0.0000       0.2768      69.4320     mm/d    precip large scale snow
      rsdt      25.5077     342.1420     437.0970     W/m2    top incoming SW radiation(down)
      rsds       6.7088     193.1820     381.1130     W/m2    SW surface(down)
      rsus       0.6190      27.0830     249.1420     W/m2    SW surface(up)
      rsut      11.7549      99.2196     275.7060     W/m2    TOA Outgoing SW Radiation(up)
      rsnt      10.0010     242.9230     385.8810     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       2.7418     166.0990     327.1200     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      61.7971     342.6060     430.8970     W/m2    LW down surface(down)
      rlus      98.3009     398.5440     529.9650     W/m2    LW up surface(up)
      rlus      98.3009     398.5440     529.9650     W/m2    olr(up)
      rlns       5.3912      55.9374     174.2020     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -185.7530       2.1984     139.1410     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -346.9130    -232.4450      30.2199     W/m2    rsns-rlns(down)
        ts     -70.7653      15.3100      37.1324        C    surface temperature
       sic       0.0000       3.7644      99.9330        %    ice cover (fraction of grid box)
       sit       0.0000       0.0433       9.3933        m    ice thickness
       tas     -65.3873      14.0032      32.8495        C    2 m temperature
       uas     -14.0059      -0.1107      15.8276      m/s    zonal wind in 10m
       vas     -12.7555       0.3001      13.9958      m/s    meridional wind in 10m
   sfcwind       0.9986       7.1943      18.1764      m/s    10m Wind Speed
      hfss    -194.4670     -17.0268     286.2480     W/m2    sensible heat flux
      hfls    -310.1120     -87.4980      63.9728     W/m2    latent heat flux
      tauu   -1399.8600      13.9573    4009.0000    mN/m2    u-stress
      tauv   -1952.6000       1.9677    1302.0500    mN/m2    v-stress
      rlus      98.3009     398.5440     529.9650     W/m2    LW up surface
  net_flux    -326.7580       5.6364     229.0540     W/m2    surface net energy flux
      rlnt    -314.8870    -240.7240    -102.9480     W/m2    net top LW radiation  (-OLR)
      rsdt      25.5077     342.1420     437.0970     W/m2    top incoming SW radiation