table_ngc4008_HP9_2026-DJF.txt Thu Feb 29 07:52:16 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       psl     949.7330    1001.5700    1029.2300      hPa    mean sea level pressure
       prw       0.2659      20.2591      54.1323    kg/m2    vertically integrated water vapor
     cllvi       0.0000      90.2650    1026.8500     g/m2    vertically integrated cloud water
     clivi       0.0000      10.1041     104.4660     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0131       0.6501    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0147       0.3240    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0535       1.4612    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.3187     148.4150     mm/d    total precipitation
      prls       0.0000       0.3235      72.7456     mm/d    precip large scale snow
      rsdt       0.0000     350.5300     487.2290     W/m2    top incoming SW radiation(down)
      rsds       0.0000     194.9170     411.2610     W/m2    SW surface(down)
      rsus       0.0000      28.1969     311.5030     W/m2    SW surface(up)
      rsut       0.0000     106.3000     324.2150     W/m2    TOA Outgoing SW Radiation(up)
      rsnt       0.0000     244.2300     425.6670     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       0.0000     166.7200     351.8180     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      85.9628     332.5290     435.8060     W/m2    LW down surface(down)
      rlus     136.8700     387.8480     549.6800     W/m2    LW up surface(up)
      rlus     136.8700     387.8480     549.6800     W/m2    olr(up)
      rlns      -6.9963      55.3194     146.5300     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -200.3360       6.7747     170.5980     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -363.9170    -221.1280       9.4074     W/m2    rsns-rlns(down)
        ts     -51.9669      13.1219      39.7868        C    surface temperature
       sic       0.0000       3.0835      99.9431        %    ice cover (fraction of grid box)
       sit       0.0000       0.0306       7.2564        m    ice thickness
       tas     -47.6437      11.8181      31.5987        C    2 m temperature
       uas     -13.7597      -0.1480      19.8172      m/s    zonal wind in 10m
       vas     -14.3466      -0.4725      11.8238      m/s    meridional wind in 10m
   sfcwind       0.6508       7.3548      22.2753      m/s    10m Wind Speed
      hfss    -250.3370     -14.5565     334.5880     W/m2    sensible heat flux
      hfls    -399.5600     -90.1716      47.6675     W/m2    latent heat flux
      tauu   -2541.1201      15.5845    5045.8501    mN/m2    u-stress
      tauv   -2793.3201      -8.4968    2224.7300    mN/m2    v-stress
      rlus     136.8700     387.8480     549.6800     W/m2    LW up surface
  net_flux    -666.0480       6.6729     280.3700     W/m2    surface net energy flux
      rlnt    -315.4780    -237.4550    -142.2510     W/m2    net top LW radiation  (-OLR)
      rsdt       0.0000     350.5300     487.2290     W/m2    top incoming SW radiation