table_ngc4008_HP9_2026-JJA.txt Thu Feb 29 07:07:18 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       psl     942.2110    1000.9200    1021.1200      hPa    mean sea level pressure
       prw       0.0699      22.6779      61.0734    kg/m2    vertically integrated water vapor
     cllvi       0.0000      92.9527    1046.5699     g/m2    vertically integrated cloud water
     clivi       0.0000       9.5512     138.7780     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0142       0.9099    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0152       0.3962    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0534       1.2224    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.3108     141.9440     mm/d    total precipitation
      prls       0.0000       0.2139      72.5314     mm/d    precip large scale snow
      rsdt       0.0000     330.4380     459.9880     W/m2    top incoming SW radiation(down)
      rsds       0.0000     181.3720     378.3210     W/m2    SW surface(down)
      rsus       0.0000      21.7892     285.6740     W/m2    SW surface(up)
      rsut       0.0000      93.2340     291.5180     W/m2    TOA Outgoing SW Radiation(up)
      rsnt       0.0000     237.2040     408.6920     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       0.0000     159.5830     331.3080     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      52.8263     350.6810     462.8550     W/m2    LW down surface(down)
      rlus      73.3768     406.9670     590.3040     W/m2    LW up surface(up)
      rlus      73.3768     406.9670     590.3040     W/m2    olr(up)
      rlns     -21.9545      56.2857     192.7380     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -186.0160      -6.1922     155.3760     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -386.8530    -247.3840     -39.5876     W/m2    rsns-rlns(down)
        ts     -83.5906      16.8717      45.2168        C    surface temperature
       sic       0.0000       2.7232      99.9643        %    ice cover (fraction of grid box)
       sit       0.0000       0.0277       6.9750        m    ice thickness
       tas     -76.0645      15.6157      42.2609        C    2 m temperature
       uas     -13.4819       0.0878      13.7720      m/s    zonal wind in 10m
       vas     -13.7287       0.6884      16.4930      m/s    meridional wind in 10m
   sfcwind       0.7051       7.2446      18.8371      m/s    10m Wind Speed
      hfss    -203.7400     -21.0191     297.4760     W/m2    sensible heat flux
      hfls    -323.9600     -90.6970     150.3340     W/m2    latent heat flux
      tauu   -1813.2800      15.0310    2938.5100    mN/m2    u-stress
      tauv   -1456.1801       7.4476    2500.7100    mN/m2    v-stress
      rlus      73.3768     406.9670     590.3040     W/m2    LW up surface
  net_flux    -399.2300      -8.4187     349.4710     W/m2    surface net energy flux
      rlnt    -343.1960    -243.3960     -82.9069     W/m2    net top LW radiation  (-OLR)
      rsdt       0.0000     330.4380     459.9880     W/m2    top incoming SW radiation