table_ngc4008_HP9_2026-MAM.txt Wed Feb 28 12:59:40 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       psl     950.1170    1001.3000    1018.6100      hPa    mean sea level pressure
       prw       0.1349      20.6409      47.4696    kg/m2    vertically integrated water vapor
     cllvi       0.0000      85.1670     731.2810     g/m2    vertically integrated cloud water
     clivi       0.0001      10.3094      69.8059     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0140       0.5649    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0143       0.3832    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0532       0.7416    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.2316     111.0860     mm/d    total precipitation
      prls       0.0000       0.2959      71.5665     mm/d    precip large scale snow
      rsdt      21.8772     338.4770     433.3240     W/m2    top incoming SW radiation(down)
      rsds      12.4386     192.4220     337.3770     W/m2    SW surface(down)
      rsus       1.1618      26.2270     267.4260     W/m2    SW surface(up)
      rsut      14.6722      96.4297     264.9200     W/m2    TOA Outgoing SW Radiation(up)
      rsnt       7.0066     242.0470     384.2590     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       2.5581     166.1950     299.3830     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      66.4722     340.6680     431.0380     W/m2    LW down surface(down)
      rlus      91.9545     397.7300     531.1230     W/m2    LW up surface(up)
      rlus      91.9545     397.7300     531.1230     W/m2    olr(up)
      rlns      -2.4857      57.0618     145.0850     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -174.1470       2.6064     135.3800     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -335.3580    -231.5350       7.1210     W/m2    rsns-rlns(down)
        ts     -72.9013      15.1304      37.2877        C    surface temperature
       sic       0.0000       2.8513      99.9972        %    ice cover (fraction of grid box)
       sit       0.0000       0.0603       9.5732        m    ice thickness
       tas     -66.9970      13.7950      35.4123        C    2 m temperature
       uas     -14.1431      -0.1237      19.3359      m/s    zonal wind in 10m
       vas     -13.6753      -0.0704      14.4758      m/s    meridional wind in 10m
   sfcwind       1.1217       7.0792      21.3333      m/s    10m Wind Speed
      hfss    -189.5180     -19.3999     258.2630     W/m2    sensible heat flux
      hfls    -290.3260     -88.0681      31.7716     W/m2    latent heat flux
      tauu   -2098.3799      13.0589    4622.6001    mN/m2    u-stress
      tauv   -2190.8401      -0.2555    1528.0000    mN/m2    v-stress
      rlus      91.9545     397.7300     531.1230     W/m2    LW up surface
  net_flux    -339.3620       1.6647     350.0940     W/m2    surface net energy flux
      rlnt    -316.1860    -239.4400    -104.6930     W/m2    net top LW radiation  (-OLR)
      rsdt      21.8772     338.4770     433.3240     W/m2    top incoming SW radiation