table_ngc4008_HP9_2026-SON.txt Thu Feb 29 07:33:33 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       psl     949.0260    1001.2500    1021.0900      hPa    mean sea level pressure
       prw       0.1025      21.2699      48.3277    kg/m2    vertically integrated water vapor
     cllvi       0.0000      87.2623     916.4140     g/m2    vertically integrated cloud water
     clivi       0.0000      10.0356      82.0257     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0135       0.8550    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0146       0.3898    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0528       0.7459    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.2392     146.5460     mm/d    total precipitation
      prls       0.0000       0.2742      63.9886     mm/d    precip large scale snow
      rsdt      26.0330     342.0470     436.8260     W/m2    top incoming SW radiation(down)
      rsds       5.3281     192.8090     376.6720     W/m2    SW surface(down)
      rsus       0.3730      26.6761     255.9660     W/m2    SW surface(up)
      rsut      11.4025      99.2488     273.1050     W/m2    TOA Outgoing SW Radiation(up)
      rsnt      11.8315     242.7990     384.1610     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       3.1688     166.1330     327.3300     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      60.3862     342.7910     429.4010     W/m2    LW down surface(down)
      rlus      95.0802     398.8050     529.0440     W/m2    LW up surface(up)
      rlus      95.0802     398.8050     529.0440     W/m2    olr(up)
      rlns       1.4991      56.0144     176.4670     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -188.3920       2.1925     139.3520     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -350.7770    -232.6720      44.1848     W/m2    rsns-rlns(down)
        ts     -71.9296      15.3991      37.0186        C    surface temperature
       sic       0.0000       2.8255      99.9387        %    ice cover (fraction of grid box)
       sit       0.0000       0.0280       9.8124        m    ice thickness
       tas     -66.2448      14.0891      32.1858        C    2 m temperature
       uas     -13.3788      -0.1225      18.1032      m/s    zonal wind in 10m
       vas     -14.3111       0.2760      13.6348      m/s    meridional wind in 10m
   sfcwind       0.9762       7.2119      20.0724      m/s    10m Wind Speed
      hfss    -200.8750     -17.2285     277.1240     W/m2    sensible heat flux
      hfls    -354.5560     -86.9216      61.0501     W/m2    latent heat flux
      tauu   -1478.3101      12.0967    4562.9399    mN/m2    u-stress
      tauv   -2187.3501       0.3038    1508.7300    mN/m2    v-stress
      rlus      95.0802     398.8050     529.0440     W/m2    LW up surface
  net_flux    -434.6500       5.9688     226.5910     W/m2    surface net energy flux
      rlnt    -314.5110    -240.6060    -101.7370     W/m2    net top LW radiation  (-OLR)
      rsdt      26.0330     342.0470     436.8260     W/m2    top incoming SW radiation