table_ngc4008_HP9_2027-JJA.txt Mon Mar 04 06:35:37 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       psl     947.9940    1000.9300    1019.1300      hPa    mean sea level pressure
       prw       0.0787      22.7853      60.4880    kg/m2    vertically integrated water vapor
     cllvi       0.0000      92.1337    1116.5100     g/m2    vertically integrated cloud water
     clivi       0.0000       9.5991     139.3870     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0144       1.0367    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0153       0.3431    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0536       1.1182    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.3198     148.6420     mm/d    total precipitation
      prls       0.0000       0.2177      73.0690     mm/d    precip large scale snow
      rsdt       0.0000     330.3770     460.0830     W/m2    top incoming SW radiation(down)
      rsds       0.0000     182.0150     387.3460     W/m2    SW surface(down)
      rsus       0.0000      22.4165     305.0340     W/m2    SW surface(up)
      rsut       0.0000      93.1233     290.4710     W/m2    TOA Outgoing SW Radiation(up)
      rsnt       0.0000     237.2530     407.4770     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       0.0000     159.5980     328.1150     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      55.1708     351.2900     457.1610     W/m2    LW down surface(down)
      rlus      74.0220     407.4750     573.4840     W/m2    LW up surface(up)
      rlus      74.0220     407.4750     573.4840     W/m2    olr(up)
      rlns     -18.3897      56.1854     169.5350     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -186.3890      -6.3104     160.4960     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -384.3630    -247.8770     -35.1170     W/m2    rsns-rlns(down)
        ts     -83.0912      16.9775      43.0575        C    surface temperature
       sic       0.0000       3.1566      99.9799        %    ice cover (fraction of grid box)
       sit       0.0000       0.0332       6.9679        m    ice thickness
       tas     -75.5767      15.7074      41.4672        C    2 m temperature
       uas     -14.6609       0.1155      17.2137      m/s    zonal wind in 10m
       vas     -13.9055       0.6840      16.5842      m/s    meridional wind in 10m
   sfcwind       0.8186       7.2051      20.0974      m/s    10m Wind Speed
      hfss    -201.0180     -20.9346     276.6960     W/m2    sensible heat flux
      hfls    -323.8920     -90.8763     148.4040     W/m2    latent heat flux
      tauu   -1678.8600      15.3101    4118.6401    mN/m2    u-stress
      tauv   -1838.0200       7.3519    2560.5400    mN/m2    v-stress
      rlus      74.0220     407.4750     573.4840     W/m2    LW up surface
  net_flux    -399.3140      -8.3982     351.2800     W/m2    surface net energy flux
      rlnt    -341.1590    -243.5640     -84.1051     W/m2    net top LW radiation  (-OLR)
      rsdt       0.0000     330.3770     460.0830     W/m2    top incoming SW radiation