table_ngc4008_HP9_2027-MAM.txt Thu Feb 29 08:10:46 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       psl     954.3620    1001.2700    1019.4500      hPa    mean sea level pressure
       prw       0.1324      20.5753      47.7685    kg/m2    vertically integrated water vapor
     cllvi       0.0000      82.8654     672.0320     g/m2    vertically integrated cloud water
     clivi       0.0025      10.3963      73.8225     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0141       0.6266    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0142       0.3687    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0529       0.8482    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.2121     123.5990     mm/d    total precipitation
      prls       0.0000       0.2945      51.7467     mm/d    precip large scale snow
      rsdt      22.3750     338.4840     433.1760     W/m2    top incoming SW radiation(down)
      rsds      12.0400     193.5100     342.8450     W/m2    SW surface(down)
      rsus       1.2629      26.9885     270.7260     W/m2    SW surface(up)
      rsut      13.1858      96.2580     263.2610     W/m2    TOA Outgoing SW Radiation(up)
      rsnt       7.0883     242.2260     384.7050     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       2.3954     166.5220     307.9490     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      65.2474     340.1210     431.7430     W/m2    LW down surface(down)
      rlus      90.8512     397.6360     523.6070     W/m2    LW up surface(up)
      rlus      90.8512     397.6360     523.6070     W/m2    olr(up)
      rlns       6.3104      57.5150     146.6690     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -168.3350       2.9613     138.8310     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -333.6730    -231.1150       7.4895     W/m2    rsns-rlns(down)
        ts     -73.4144      15.0646      36.6165        C    surface temperature
       sic       0.0000       3.2098      99.9982        %    ice cover (fraction of grid box)
       sit       0.0000       0.0458       7.2953        m    ice thickness
       tas     -67.4525      13.7244      34.3647        C    2 m temperature
       uas     -13.7968      -0.0823      13.8786      m/s    zonal wind in 10m
       vas     -10.5682      -0.0416      14.9787      m/s    meridional wind in 10m
   sfcwind       1.1056       6.9918      18.3226      m/s    10m Wind Speed
      hfss    -188.7420     -19.4109     203.5540     W/m2    sensible heat flux
      hfls    -276.6520     -87.5784      17.4877     W/m2    latent heat flux
      tauu   -1849.5300      12.1582    3325.2900    mN/m2    u-stress
      tauv   -1802.5601      -0.3288    1731.6500    mN/m2    v-stress
      rlus      90.8512     397.6360     523.6070     W/m2    LW up surface
  net_flux    -324.3390       2.0173     277.2510     W/m2    surface net energy flux
      rlnt    -320.0920    -239.2650    -104.4430     W/m2    net top LW radiation  (-OLR)
      rsdt      22.3750     338.4840     433.1760     W/m2    top incoming SW radiation