table_ngc4008_HP9_2027-SON.txt Mon Mar 04 07:16:25 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       psl     944.5490    1001.2400    1021.7900      hPa    mean sea level pressure
       prw       0.1188      21.4545      50.0373    kg/m2    vertically integrated water vapor
     cllvi       0.0000      88.6416     828.6620     g/m2    vertically integrated cloud water
     clivi       0.0000      10.0812      86.4090     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0136       0.8471    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0148       0.3701    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0529       0.9798    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.2641     142.8650     mm/d    total precipitation
      prls       0.0000       0.2750      66.5459     mm/d    precip large scale snow
      rsdt      26.5738     341.9900     436.5990     W/m2    top incoming SW radiation(down)
      rsds       6.7520     192.0510     383.3930     W/m2    SW surface(down)
      rsus       0.4728      26.4271     254.4090     W/m2    SW surface(up)
      rsut      11.3230      99.5927     276.4560     W/m2    TOA Outgoing SW Radiation(up)
      rsnt      10.4014     242.3980     384.2230     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       2.4717     165.6240     328.3040     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      63.4301     343.2110     431.3540     W/m2    LW down surface(down)
      rlus      97.9180     398.9730     528.0220     W/m2    LW up surface(up)
      rlus      97.9180     398.9730     528.0220     W/m2    olr(up)
      rlns       4.4466      55.7621     177.6730     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -179.4590       1.6999     137.3180     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -350.5910    -233.3490      42.2251     W/m2    rsns-rlns(down)
        ts     -70.6010      15.4258      36.8744        C    surface temperature
       sic       0.0000       3.3183      99.8497        %    ice cover (fraction of grid box)
       sit       0.0000       0.0344       8.8664        m    ice thickness
       tas     -65.1159      14.1056      32.8629        C    2 m temperature
       uas     -14.7913      -0.0365      17.3137      m/s    zonal wind in 10m
       vas     -12.7046       0.2873      14.2319      m/s    meridional wind in 10m
   sfcwind       0.9943       7.2231      19.0452      m/s    10m Wind Speed
      hfss    -202.4750     -16.9750     242.2100     W/m2    sensible heat flux
      hfls    -288.5500     -87.5358      74.6204     W/m2    latent heat flux
      tauu   -1531.8700      15.8433    4455.7100    mN/m2    u-stress
      tauv   -1964.4200       1.6608    1674.3700    mN/m2    v-stress
      rlus      97.9180     398.9730     528.0220     W/m2    LW up surface
  net_flux    -323.6370       5.3507     235.9660     W/m2    surface net energy flux
      rlnt    -313.1270    -240.6980    -102.5390     W/m2    net top LW radiation  (-OLR)
      rsdt      26.5738     341.9900     436.5990     W/m2    top incoming SW radiation