table_ngc4008_HP9_2030-DJF.txt Mon Mar 04 10:16:19 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       psl     953.7160    1001.6000    1031.1801      hPa    mean sea level pressure
       prw       0.2850      20.4187      52.9031    kg/m2    vertically integrated water vapor
     cllvi       0.0000      90.8764    1198.7400     g/m2    vertically integrated cloud water
     clivi       0.0000      10.0082     100.3110     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0132       0.5072    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0147       0.2875    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0528       1.4059    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.3087     123.5140     mm/d    total precipitation
      prls       0.0000       0.3279      76.2822     mm/d    precip large scale snow
      rsdt       0.0000     350.4630     487.0970     W/m2    top incoming SW radiation(down)
      rsds       0.0000     195.5710     403.8870     W/m2    SW surface(down)
      rsus       0.0000      28.1165     310.7390     W/m2    SW surface(up)
      rsut       0.0000     105.4330     324.0460     W/m2    TOA Outgoing SW Radiation(up)
      rsnt       0.0000     245.0300     424.7190     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       0.0000     167.4540     352.7150     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      88.1647     333.4740     434.5400     W/m2    LW down surface(down)
      rlus     141.3270     388.9910     539.3550     W/m2    LW up surface(up)
      rlus     141.3270     388.9910     539.3550     W/m2    olr(up)
      rlns      -9.3428      55.5166     150.9530     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -190.3290       7.3182     166.1950     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -392.8470    -221.5360       7.8734     W/m2    rsns-rlns(down)
        ts     -49.9385      13.3850      38.3830        C    surface temperature
       sic       0.0000       3.1175      99.9972        %    ice cover (fraction of grid box)
       sit       0.0000       0.0347       8.7969        m    ice thickness
       tas     -45.6608      12.0594      31.3956        C    2 m temperature
       uas     -13.7863      -0.1991      20.2723      m/s    zonal wind in 10m
       vas     -17.2990      -0.4941      15.1761      m/s    meridional wind in 10m
   sfcwind       0.6946       7.2689      22.5086      m/s    10m Wind Speed
      hfss    -250.5960     -14.6601     371.7900     W/m2    sensible heat flux
      hfls    -415.2730     -89.9984      80.1424     W/m2    latent heat flux
      tauu   -2768.8601      16.9534    4528.5400    mN/m2    u-stress
      tauv   -3097.7600      -5.2178    2399.1799    mN/m2    v-stress
      rlus     141.3270     388.9910     539.3550     W/m2    LW up surface
  net_flux    -643.8780       7.2791     282.0110     W/m2    surface net energy flux
      rlnt    -313.6560    -237.7120    -133.3530     W/m2    net top LW radiation  (-OLR)
      rsdt       0.0000     350.4630     487.0970     W/m2    top incoming SW radiation