table_ngc4008_HP9_2030-JJA.txt Mon Mar 04 08:38:15 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       psl     939.7010    1000.8900    1021.1000      hPa    mean sea level pressure
       prw       0.0771      22.9204      60.3694    kg/m2    vertically integrated water vapor
     cllvi       0.0000      93.4273    1128.8101     g/m2    vertically integrated cloud water
     clivi       0.0000       9.6479     138.8830     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0141       0.8238    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0153       0.3684    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0534       1.1625    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.3041     133.9130     mm/d    total precipitation
      prls       0.0000       0.2176      78.1266     mm/d    precip large scale snow
      rsdt       0.0000     330.3080     459.7700     W/m2    top incoming SW radiation(down)
      rsds       0.0000     181.6310     375.6310     W/m2    SW surface(down)
      rsus       0.0000      22.1750     280.9310     W/m2    SW surface(up)
      rsut       0.0000      93.0870     286.9390     W/m2    TOA Outgoing SW Radiation(up)
      rsnt       0.0000     237.2210     407.7830     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       0.0000     159.4560     320.5460     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      55.1167     351.6970     459.5780     W/m2    LW down surface(down)
      rlus      74.5081     407.9680     589.4560     W/m2    LW up surface(up)
      rlus      74.5081     407.9680     589.4560     W/m2    olr(up)
      rlns     -19.5356      56.2708     190.1010     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -188.4470      -6.3556     154.3040     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -388.2390    -248.5120     -37.9327     W/m2    rsns-rlns(down)
        ts     -82.7635      17.0662      45.1489        C    surface temperature
       sic       0.0000       3.0911      99.9784        %    ice cover (fraction of grid box)
       sit       0.0000       0.0328       7.1439        m    ice thickness
       tas     -75.1538      15.8118      42.0856        C    2 m temperature
       uas     -16.1900       0.0782      15.5840      m/s    zonal wind in 10m
       vas     -13.2203       0.6538      16.5775      m/s    meridional wind in 10m
   sfcwind       0.9191       7.2407      18.0949      m/s    10m Wind Speed
      hfss    -208.7840     -21.1113     263.5550     W/m2    sensible heat flux
      hfls    -325.1220     -90.3027     153.3840     W/m2    latent heat flux
      tauu   -1800.4301      15.4697    3994.8999    mN/m2    u-stress
      tauv   -1830.0900       7.2448    2310.1699    mN/m2    v-stress
      rlus      74.5081     407.9680     589.4560     W/m2    LW up surface
  net_flux    -413.7260      -8.2288     364.0410     W/m2    surface net energy flux
      rlnt    -333.1840    -243.5760     -84.8359     W/m2    net top LW radiation  (-OLR)
      rsdt       0.0000     330.3080     459.7700     W/m2    top incoming SW radiation