table_ngc4008_HP9_2030-MAM.txt Mon Mar 04 07:56:02 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       psl     953.7100    1001.2800    1022.0600      hPa    mean sea level pressure
       prw       0.1305      20.8387      47.4118    kg/m2    vertically integrated water vapor
     cllvi       0.0000      83.0903     712.8920     g/m2    vertically integrated cloud water
     clivi       0.0006      10.3826      67.3807     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0140       0.6046    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0143       0.3301    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0530       0.9693    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.2191     119.1440     mm/d    total precipitation
      prls       0.0000       0.2913      58.9621     mm/d    precip large scale snow
      rsdt      22.0217     338.4270     433.0920     W/m2    top incoming SW radiation(down)
      rsds      12.9696     193.9890     337.9230     W/m2    SW surface(down)
      rsus       1.2918      26.6607     265.8580     W/m2    SW surface(up)
      rsut      14.2491      95.3847     261.7900     W/m2    TOA Outgoing SW Radiation(up)
      rsnt       7.1140     243.0420     383.6730     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       2.5909     167.3290     307.5860     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      65.2136     341.2110     429.5790     W/m2    LW down surface(down)
      rlus      92.0851     398.9300     524.1690     W/m2    LW up surface(up)
      rlus      92.0851     398.9300     524.1690     W/m2    olr(up)
      rlns       0.4933      57.7193     147.0670     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -169.1460       3.4825     137.6310     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -335.2990    -231.6010       4.9682     W/m2    rsns-rlns(down)
        ts     -72.7458      15.3428      36.7865        C    surface temperature
       sic       0.0000       3.0598      99.9956        %    ice cover (fraction of grid box)
       sit       0.0000       0.0480       8.9778        m    ice thickness
       tas     -66.9953      14.0324      35.2828        C    2 m temperature
       uas     -13.9199      -0.0526      16.6704      m/s    zonal wind in 10m
       vas     -13.4341      -0.1142      15.0480      m/s    meridional wind in 10m
   sfcwind       1.0679       7.0354      19.8578      m/s    10m Wind Speed
      hfss    -191.0790     -19.4611     204.1530     W/m2    sensible heat flux
      hfls    -261.8750     -87.7432      37.5753     W/m2    latent heat flux
      tauu   -1797.8500      14.9486    4191.7900    mN/m2    u-stress
      tauv   -2027.5500      -0.8073    1359.8101    mN/m2    v-stress
      rlus      92.0851     398.9300     524.1690     W/m2    LW up surface
  net_flux    -347.5960       2.4051     272.3180     W/m2    surface net energy flux
      rlnt    -319.4270    -239.5600    -104.9990     W/m2    net top LW radiation  (-OLR)
      rsdt      22.0217     338.4270     433.0920     W/m2    top incoming SW radiation