table_ngc4008_HP9_2030-SON.txt Mon Mar 04 09:17:11 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       psl     946.8550    1001.2300    1022.7600      hPa    mean sea level pressure
       prw       0.1068      21.5957      48.9357    kg/m2    vertically integrated water vapor
     cllvi       0.0000      85.8679     824.8390     g/m2    vertically integrated cloud water
     clivi       0.0000      10.0076      76.2369     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0137       0.8707    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0146       0.4290    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0522       0.9071    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.2129     145.8390     mm/d    total precipitation
      prls       0.0000       0.2680      74.9645     mm/d    precip large scale snow
      rsdt      25.9563     341.9490     436.7180     W/m2    top incoming SW radiation(down)
      rsds       6.4359     193.1510     385.3650     W/m2    SW surface(down)
      rsus       0.5257      26.6697     264.2410     W/m2    SW surface(up)
      rsut      11.0555      98.6102     273.4320     W/m2    TOA Outgoing SW Radiation(up)
      rsnt      10.7039     243.3390     383.6430     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       2.5824     166.4810     328.7030     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      60.9006     343.3040     428.0740     W/m2    LW down surface(down)
      rlus      99.1004     399.7130     526.8390     W/m2    LW up surface(up)
      rlus      99.1004     399.7130     526.8390     W/m2    olr(up)
      rlns       5.6793      56.4085     180.0570     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -182.7010       2.8618     139.1800     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -354.2020    -233.2320      40.6335     W/m2    rsns-rlns(down)
        ts     -69.7812      15.5366      36.6997        C    surface temperature
       sic       0.0000       3.3128      99.8909        %    ice cover (fraction of grid box)
       sit       0.0000       0.0336       8.1804        m    ice thickness
       tas     -64.6135      14.2371      33.4913        C    2 m temperature
       uas     -13.8826      -0.0864      18.3820      m/s    zonal wind in 10m
       vas     -13.2040       0.3087      13.0479      m/s    meridional wind in 10m
   sfcwind       0.9285       7.1767      20.5257      m/s    10m Wind Speed
      hfss    -200.0290     -17.3791     303.3630     W/m2    sensible heat flux
      hfls    -323.0930     -86.2853      60.9114     W/m2    latent heat flux
      tauu   -1654.3199      15.7122    4794.0200    mN/m2    u-stress
      tauv   -2173.5200       2.4741    1244.2500    mN/m2    v-stress
      rlus      99.1004     399.7130     526.8390     W/m2    LW up surface
  net_flux    -371.5730       6.4080     210.7690     W/m2    surface net energy flux
      rlnt    -305.1040    -240.4770    -104.1790     W/m2    net top LW radiation  (-OLR)
      rsdt      25.9563     341.9490     436.7180     W/m2    top incoming SW radiation