table_ngc4008_HP9_2031-DJF.txt Tue Mar 05 09:24:57 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       psl     958.7250    1001.6200    1026.2600      hPa    mean sea level pressure
       prw       0.2725      20.3956      52.3313    kg/m2    vertically integrated water vapor
     cllvi       0.0000      91.7900    1156.6700     g/m2    vertically integrated cloud water
     clivi       0.0000       9.9373     104.3540     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0128       0.6564    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0147       0.3403    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0533       1.6374    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.3066     141.3500     mm/d    total precipitation
      prls       0.0000       0.3335      95.4844     mm/d    precip large scale snow
      rsdt       0.0000     350.4830     487.3140     W/m2    top incoming SW radiation(down)
      rsds       0.0000     194.6760     395.5690     W/m2    SW surface(down)
      rsus       0.0000      27.9840     307.8230     W/m2    SW surface(up)
      rsut       0.0000     106.0420     323.6970     W/m2    TOA Outgoing SW Radiation(up)
      rsnt       0.0000     244.4410     425.2620     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       0.0000     166.6920     347.5990     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      97.0599     333.5450     435.5000     W/m2    LW down surface(down)
      rlus     137.0490     388.6130     519.8420     W/m2    LW up surface(up)
      rlus     137.0490     388.6130     519.8420     W/m2    olr(up)
      rlns      -9.8771      55.0676     152.5150     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -188.6090       6.5971     164.9450     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -390.4740    -221.9210      -3.9072     W/m2    rsns-rlns(down)
        ts     -51.7165      13.3216      35.6405        C    surface temperature
       sic       0.0000       3.2079      99.9910        %    ice cover (fraction of grid box)
       sit       0.0000       0.0346       7.8818        m    ice thickness
       tas     -47.2756      12.0266      32.2369        C    2 m temperature
       uas     -16.8961      -0.4537      21.6677      m/s    zonal wind in 10m
       vas     -14.7035      -0.4767      11.9351      m/s    meridional wind in 10m
   sfcwind       0.4991       7.3303      24.4113      m/s    10m Wind Speed
      hfss    -245.3050     -14.4042     469.9880     W/m2    sensible heat flux
      hfls    -411.1180     -89.7768      57.5419     W/m2    latent heat flux
      tauu   -3282.8000      13.7242    5602.8398    mN/m2    u-stress
      tauv   -3639.7400      -7.2579    1966.1100    mN/m2    v-stress
      rlus     137.0490     388.6130     519.8420     W/m2    LW up surface
  net_flux    -594.9690       7.4433     282.9410     W/m2    surface net energy flux
      rlnt    -315.5080    -237.8440    -130.6180     W/m2    net top LW radiation  (-OLR)
      rsdt       0.0000     350.4830     487.3140     W/m2    top incoming SW radiation