table_ngc4008_HP9_2031-JJA.txt Tue Mar 05 07:06:53 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       psl     950.5070    1000.9300    1020.3200      hPa    mean sea level pressure
       prw       0.0962      22.9292      60.8684    kg/m2    vertically integrated water vapor
     cllvi       0.0000      91.3765    1093.9500     g/m2    vertically integrated cloud water
     clivi       0.0000       9.6202     137.5680     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0143       1.0721    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0151       0.3334    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0533       1.1041    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.2850     142.0450     mm/d    total precipitation
      prls       0.0000       0.2159      75.0394     mm/d    precip large scale snow
      rsdt       0.0000     330.2740     459.9010     W/m2    top incoming SW radiation(down)
      rsds       0.0000     182.2060     381.8420     W/m2    SW surface(down)
      rsus       0.0000      22.1861     290.2920     W/m2    SW surface(up)
      rsut       0.0000      92.4680     285.7460     W/m2    TOA Outgoing SW Radiation(up)
      rsnt       0.0000     237.8060     408.2630     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       0.0000     160.0200     328.8160     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      59.8553     351.6430     457.8880     W/m2    LW down surface(down)
      rlus      77.9919     408.1880     592.3770     W/m2    LW up surface(up)
      rlus      77.9919     408.1880     592.3770     W/m2    olr(up)
      rlns     -16.1525      56.5443     190.5430     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -189.4310      -5.5346     158.6680     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -383.8320    -248.1670     -43.2076     W/m2    rsns-rlns(down)
        ts     -80.6579      17.1237      45.5514        C    surface temperature
       sic       0.0000       3.1317      99.9591        %    ice cover (fraction of grid box)
       sit       0.0000       0.0304       6.5072        m    ice thickness
       tas     -73.1370      15.8514      42.1801        C    2 m temperature
       uas     -15.5917       0.0764      15.7971      m/s    zonal wind in 10m
       vas     -14.3549       0.6755      16.5768      m/s    meridional wind in 10m
   sfcwind       0.8496       7.1745      19.1255      m/s    10m Wind Speed
      hfss    -209.3390     -21.2780     282.2240     W/m2    sensible heat flux
      hfls    -306.8040     -90.0954     192.0580     W/m2    latent heat flux
      tauu   -1643.9000      14.2773    3506.2500    mN/m2    u-stress
      tauv   -1797.8101       7.9064    2226.3301    mN/m2    v-stress
      rlus      77.9919     408.1880     592.3770     W/m2    LW up surface
  net_flux    -415.0140      -7.8975     436.1930     W/m2    surface net energy flux
      rlnt    -333.1880    -243.3410     -87.9015     W/m2    net top LW radiation  (-OLR)
      rsdt       0.0000     330.2740     459.9010     W/m2    top incoming SW radiation