table_ngc4008_HP9_2031-MAM.txt Tue Mar 05 06:44:11 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       psl     953.5000    1001.3100    1017.1700      hPa    mean sea level pressure
       prw       0.1440      20.7742      47.1122    kg/m2    vertically integrated water vapor
     cllvi       0.0000      83.7403     736.1060     g/m2    vertically integrated cloud water
     clivi       0.0000      10.3731      64.9803     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0142       0.6019    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0142       0.3458    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0533       0.8055    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.2162     123.4120     mm/d    total precipitation
      prls       0.0000       0.2797      56.3174     mm/d    precip large scale snow
      rsdt      22.2998     338.3670     433.0460     W/m2    top incoming SW radiation(down)
      rsds      12.6272     192.9480     337.8780     W/m2    SW surface(down)
      rsus       1.1677      26.5988     270.0430     W/m2    SW surface(up)
      rsut      12.4905      96.0999     264.3540     W/m2    TOA Outgoing SW Radiation(up)
      rsnt       7.0318     242.2670     384.6770     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       2.5006     166.3490     306.4220     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      66.5179     341.3230     427.5570     W/m2    LW down surface(down)
      rlus      92.8663     398.3250     524.8270     W/m2    LW up surface(up)
      rlus      92.8663     398.3250     524.8270     W/m2    olr(up)
      rlns      -0.6786      57.0019     145.1140     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -170.0110       3.2400     137.7890     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -337.8450    -231.9760       8.5101     W/m2    rsns-rlns(down)
        ts     -72.4371      15.2287      36.6660        C    surface temperature
       sic       0.0000       3.0316      99.9984        %    ice cover (fraction of grid box)
       sit       0.0000       0.0451       9.4188        m    ice thickness
       tas     -66.6669      13.8874      33.8649        C    2 m temperature
       uas     -13.8096      -0.1569      15.3357      m/s    zonal wind in 10m
       vas     -12.5574      -0.0646      14.8856      m/s    meridional wind in 10m
   sfcwind       1.0161       6.9500      18.7055      m/s    10m Wind Speed
      hfss    -192.8510     -19.5516     201.0870     W/m2    sensible heat flux
      hfls    -258.2840     -87.5172      30.2216     W/m2    latent heat flux
      tauu   -1758.6700       8.9886    3574.3899    mN/m2    u-stress
      tauv   -1705.7900      -1.5433    1419.0300    mN/m2    v-stress
      rlus      92.8663     398.3250     524.8270     W/m2    LW up surface
  net_flux    -342.2870       2.2782     309.7410     W/m2    surface net energy flux
      rlnt    -318.0890    -239.0270    -105.3440     W/m2    net top LW radiation  (-OLR)
      rsdt      22.2998     338.3670     433.0460     W/m2    top incoming SW radiation