table_ngc4008_HP9_2031-SON.txt Tue Mar 05 07:28:35 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       psl     946.3430    1001.2300    1021.4700      hPa    mean sea level pressure
       prw       0.1331      21.7602      49.1817    kg/m2    vertically integrated water vapor
     cllvi       0.0000      87.7052     760.6700     g/m2    vertically integrated cloud water
     clivi       0.0000      10.0696      81.1153     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0135       0.7902    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0149       0.3998    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0526       0.7690    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.2606     145.4240     mm/d    total precipitation
      prls       0.0000       0.2671      66.4671     mm/d    precip large scale snow
      rsdt      26.4974     341.8950     436.4960     W/m2    top incoming SW radiation(down)
      rsds       6.7785     192.5650     379.0750     W/m2    SW surface(down)
      rsus       0.4997      26.7130     253.1510     W/m2    SW surface(up)
      rsut       9.8251      99.1415     272.8540     W/m2    TOA Outgoing SW Radiation(up)
      rsnt      10.9043     242.7540     383.1100     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       2.9556     165.8520     326.9740     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      66.2756     343.8850     431.1060     W/m2    LW down surface(down)
      rlus     102.6730     399.5650     529.1430     W/m2    LW up surface(up)
      rlus     102.6730     399.5650     529.1430     W/m2    olr(up)
      rlns       4.2876      55.6796     179.1300     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -181.1750       2.2532     138.7890     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -354.3050    -233.7130      25.5649     W/m2    rsns-rlns(down)
        ts     -67.9903      15.5315      37.0357        C    surface temperature
       sic       0.0000       3.4284      99.7976        %    ice cover (fraction of grid box)
       sit       0.0000       0.0325       9.0038        m    ice thickness
       tas     -62.7424      14.2395      33.0690        C    2 m temperature
       uas     -15.8193      -0.1904      16.5508      m/s    zonal wind in 10m
       vas     -12.3432       0.2791      15.7916      m/s    meridional wind in 10m
   sfcwind       0.9303       7.2179      18.8340      m/s    10m Wind Speed
      hfss    -202.6510     -16.9377     340.2340     W/m2    sensible heat flux
      hfls    -360.2610     -87.4662      75.6590     W/m2    latent heat flux
      tauu   -1629.1899      12.9913    4336.8999    mN/m2    u-stress
      tauv   -1913.0500       0.6273    1432.2500    mN/m2    v-stress
      rlus     102.6730     399.5650     529.1430     W/m2    LW up surface
  net_flux    -295.6080       5.7686     213.2840     W/m2    surface net energy flux
      rlnt    -311.4780    -240.5010    -107.0840     W/m2    net top LW radiation  (-OLR)
      rsdt      26.4974     341.8950     436.4960     W/m2    top incoming SW radiation