table_ngc4008_HP9_2032-DJF.txt Wed Mar 06 06:57:42 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       psl     952.8410    1001.5900    1024.8101      hPa    mean sea level pressure
       prw       0.2932      20.4808      53.1725    kg/m2    vertically integrated water vapor
     cllvi       0.0000      90.7929     998.6440     g/m2    vertically integrated cloud water
     clivi       0.0000      10.0099     110.1550     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0130       0.5329    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0148       0.3228    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0532       1.5294    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.3112     132.1480     mm/d    total precipitation
      prls       0.0000       0.3269      72.2274     mm/d    precip large scale snow
      rsdt       0.0000     350.4820     486.7010     W/m2    top incoming SW radiation(down)
      rsds       0.0000     195.2620     418.4520     W/m2    SW surface(down)
      rsus       0.0000      28.0166     307.6060     W/m2    SW surface(up)
      rsut       0.0000     105.4890     321.9460     W/m2    TOA Outgoing SW Radiation(up)
      rsnt       0.0000     244.9940     428.0920     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       0.0000     167.2450     360.2570     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      90.9263     333.4340     435.3640     W/m2    LW down surface(down)
      rlus     146.7690     388.5300     525.8700     W/m2    LW up surface(up)
      rlus     146.7690     388.5300     525.8700     W/m2    olr(up)
      rlns      -5.8524      55.0953     145.8020     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -192.8280       7.3828     162.8970     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -367.1020    -221.2850      16.8343     W/m2    rsns-rlns(down)
        ts     -47.8878      13.2420      36.5900        C    surface temperature
       sic       0.0000       3.1375      99.9749        %    ice cover (fraction of grid box)
       sit       0.0000       0.0340       8.7764        m    ice thickness
       tas     -44.0086      11.9551      32.0951        C    2 m temperature
       uas     -14.9521      -0.3305      18.8945      m/s    zonal wind in 10m
       vas     -13.6695      -0.4905      11.2345      m/s    meridional wind in 10m
   sfcwind       0.8480       7.3357      20.7340      m/s    10m Wind Speed
      hfss    -252.0320     -14.4634     384.5090     W/m2    sensible heat flux
      hfls    -379.5030     -90.0257      54.1228     W/m2    latent heat flux
      tauu   -2615.9600      12.4913    4473.7998    mN/m2    u-stress
      tauv   -2901.0901      -7.4813    2193.5801    mN/m2    v-stress
      rlus     146.7690     388.5300     525.8700     W/m2    LW up surface
  net_flux    -594.6780       7.6606     287.4750     W/m2    surface net energy flux
      rlnt    -316.3770    -237.6110    -133.3230     W/m2    net top LW radiation  (-OLR)
      rsdt       0.0000     350.4820     486.7010     W/m2    top incoming SW radiation