table_ngc4008_HP9_2032-JJA.txt Wed Mar 06 06:16:54 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       psl     946.9850    1000.9200    1018.7600      hPa    mean sea level pressure
       prw       0.0932      22.8877      61.5834    kg/m2    vertically integrated water vapor
     cllvi       0.0000      92.3858    1064.5699     g/m2    vertically integrated cloud water
     clivi       0.0000       9.6142     143.2020     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0142       0.9941    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0152       0.3562    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0535       1.4412    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.2844     142.3240     mm/d    total precipitation
      prls       0.0000       0.2137      70.9980     mm/d    precip large scale snow
      rsdt       0.0000     330.2950     459.3610     W/m2    top incoming SW radiation(down)
      rsds       0.0000     182.0210     373.3310     W/m2    SW surface(down)
      rsus       0.0000      22.1512     285.5680     W/m2    SW surface(up)
      rsut       0.0000      92.6196     293.2630     W/m2    TOA Outgoing SW Radiation(up)
      rsnt       0.0000     237.6760     407.7330     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       0.0000     159.8700     325.4410     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      58.8359     351.9340     462.1700     W/m2    LW down surface(down)
      rlus      77.3179     408.3730     603.0670     W/m2    LW up surface(up)
      rlus      77.3179     408.3730     603.0670     W/m2    olr(up)
      rlns     -17.4833      56.4387     203.5220     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -183.8470      -5.7860     158.4270     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -388.5990    -248.5030     -39.4115     W/m2    rsns-rlns(down)
        ts     -81.0721      17.1480      46.9433        C    surface temperature
       sic       0.0000       3.0616      99.9451        %    ice cover (fraction of grid box)
       sit       0.0000       0.0314       7.7544        m    ice thickness
       tas     -73.7921      15.8966      42.2501        C    2 m temperature
       uas     -16.9189       0.1180      13.7646      m/s    zonal wind in 10m
       vas     -14.2663       0.6944      17.7240      m/s    meridional wind in 10m
   sfcwind       0.9697       7.2265      18.9024      m/s    10m Wind Speed
      hfss    -204.6830     -21.3953     306.5720     W/m2    sensible heat flux
      hfls    -322.3260     -89.9007     144.8550     W/m2    latent heat flux
      tauu   -1813.6300      15.3914    2874.6399    mN/m2    u-stress
      tauv   -1593.6200       7.4530    2546.5500    mN/m2    v-stress
      rlus      77.3179     408.3730     603.0670     W/m2    LW up surface
  net_flux    -415.6420      -7.8647     342.8880     W/m2    surface net energy flux
      rlnt    -342.4840    -243.4620     -86.8375     W/m2    net top LW radiation  (-OLR)
      rsdt       0.0000     330.2950     459.3610     W/m2    top incoming SW radiation