table_ngc4008_HP9_2032-MAM.txt Tue Mar 05 17:10:04 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       psl     955.0680    1001.2800    1018.4100      hPa    mean sea level pressure
       prw       0.1468      20.7576      47.9574    kg/m2    vertically integrated water vapor
     cllvi       0.0000      84.0275     720.9150     g/m2    vertically integrated cloud water
     clivi       0.0029      10.3955      56.9187     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0139       0.5230    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0143       0.3443    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0537       0.7803    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.2286     124.9140     mm/d    total precipitation
      prls       0.0000       0.2923      59.8202     mm/d    precip large scale snow
      rsdt      20.7085     338.2360     433.3900     W/m2    top incoming SW radiation(down)
      rsds      10.4299     193.1170     334.9600     W/m2    SW surface(down)
      rsus       1.3564      26.5199     267.8780     W/m2    SW surface(up)
      rsut      13.7498      95.7947     262.8800     W/m2    TOA Outgoing SW Radiation(up)
      rsnt       6.4459     242.4420     383.7410     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       2.0761     166.5970     300.5960     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      66.8421     341.4380     429.8250     W/m2    LW down surface(down)
      rlus      96.6109     398.9910     530.2760     W/m2    LW up surface(up)
      rlus      96.6109     398.9910     530.2760     W/m2    olr(up)
      rlns       1.5859      57.5527     146.7320     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -171.5510       2.9837     135.8110     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -339.8440    -232.3940       0.4207     W/m2    rsns-rlns(down)
        ts     -70.3664      15.3725      37.1570        C    surface temperature
       sic       0.0000       3.0766      99.9937        %    ice cover (fraction of grid box)
       sit       0.0000       0.0484       9.7142        m    ice thickness
       tas     -64.8892      14.0522      35.4514        C    2 m temperature
       uas     -13.3181      -0.0718      15.5862      m/s    zonal wind in 10m
       vas     -11.7439       0.0196      14.3787      m/s    meridional wind in 10m
   sfcwind       1.1321       7.0742      18.2424      m/s    10m Wind Speed
      hfss    -190.1440     -19.4321     194.0840     W/m2    sensible heat flux
      hfls    -245.3880     -88.0381      27.1819     W/m2    latent heat flux
      tauu   -2019.2900      15.9378    3529.5300    mN/m2    u-stress
      tauv   -2087.5701       2.2907    1487.6899    mN/m2    v-stress
      rlus      96.6109     398.9910     530.2760     W/m2    LW up surface
  net_flux    -333.0960       1.5738     309.2850     W/m2    surface net energy flux
      rlnt    -313.5970    -239.4580    -107.1920     W/m2    net top LW radiation  (-OLR)
      rsdt      20.7085     338.2360     433.3900     W/m2    top incoming SW radiation