table_ngc4008_HP9_2032-SON.txt Wed Mar 06 06:41:14 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       psl     945.0020    1001.2300    1022.0900      hPa    mean sea level pressure
       prw       0.1214      21.5546      48.8400    kg/m2    vertically integrated water vapor
     cllvi       0.0000      88.3794     810.1830     g/m2    vertically integrated cloud water
     clivi       0.0000       9.9435      77.8996     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0134       0.9259    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0147       0.4821    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0528       0.7887    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.2448     140.7460     mm/d    total precipitation
      prls       0.0000       0.2659      62.7023     mm/d    precip large scale snow
      rsdt      24.8262     342.0250     437.1390     W/m2    top incoming SW radiation(down)
      rsds       4.6961     192.2930     382.9590     W/m2    SW surface(down)
      rsus       0.3316      26.7976     262.2620     W/m2    SW surface(up)
      rsut      11.3572      99.4867     272.2460     W/m2    TOA Outgoing SW Radiation(up)
      rsnt       9.7554     242.5390     385.1640     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       2.0645     165.4950     327.8370     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      63.4516     343.7620     429.9370     W/m2    LW down surface(down)
      rlus      99.1521     399.5770     530.0210     W/m2    LW up surface(up)
      rlus      99.1521     399.5770     530.0210     W/m2    olr(up)
      rlns       4.2958      55.8152     178.8090     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -184.0710       1.9148     139.8340     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -354.6790    -234.0810      33.8222     W/m2    rsns-rlns(down)
        ts     -69.9140      15.5260      37.1551        C    surface temperature
       sic       0.0000       3.3782      99.9615        %    ice cover (fraction of grid box)
       sit       0.0000       0.0328       8.4934        m    ice thickness
       tas     -64.5546      14.2142      33.1206        C    2 m temperature
       uas     -14.5550      -0.0789      20.6000      m/s    zonal wind in 10m
       vas     -15.6959       0.2657      14.7426      m/s    meridional wind in 10m
   sfcwind       0.8753       7.1978      22.6524      m/s    10m Wind Speed
      hfss    -204.8630     -17.1557     284.2520     W/m2    sensible heat flux
      hfls    -306.5690     -87.0244      54.5377     W/m2    latent heat flux
      tauu   -1408.7000      13.9917    5401.3901    mN/m2    u-stress
      tauv   -2705.5601       0.4646    1521.5400    mN/m2    v-stress
      rlus      99.1521     399.5770     530.0210     W/m2    LW up surface
  net_flux    -305.2950       5.5002     225.0830     W/m2    surface net energy flux
      rlnt    -310.6130    -240.6240    -102.9150     W/m2    net top LW radiation  (-OLR)
      rsdt      24.8262     342.0250     437.1390     W/m2    top incoming SW radiation