table_ngc4008_HP9_2033-DJF.txt Thu Mar 07 08:02:18 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       psl     952.1020    1001.5600    1025.2300      hPa    mean sea level pressure
       prw       0.2437      20.4455      53.3557    kg/m2    vertically integrated water vapor
     cllvi       0.0000      90.7505    1090.2400     g/m2    vertically integrated cloud water
     clivi       0.0000      10.0917     103.4580     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0131       0.5522    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0146       0.3148    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0525       1.3315    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.2819     139.4460     mm/d    total precipitation
      prls       0.0000       0.3321      74.0924     mm/d    precip large scale snow
      rsdt       0.0000     350.5400     486.9830     W/m2    top incoming SW radiation(down)
      rsds       0.0000     195.2720     405.5950     W/m2    SW surface(down)
      rsus       0.0000      28.2241     311.6690     W/m2    SW surface(up)
      rsut       0.0000     105.8060     324.3850     W/m2    TOA Outgoing SW Radiation(up)
      rsnt       0.0000     244.7350     425.1120     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       0.0000     167.0480     355.6300     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      83.5642     333.6260     434.7810     W/m2    LW down surface(down)
      rlus     141.8240     389.0540     518.0530     W/m2    LW up surface(up)
      rlus     141.8240     389.0540     518.0530     W/m2    olr(up)
      rlns      -7.8888      55.4280     151.7380     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -189.8400       7.6061     162.6310     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -397.8800    -222.0060      -2.2184     W/m2    rsns-rlns(down)
        ts     -49.8325      13.3932      35.4760        C    surface temperature
       sic       0.0000       3.1804      99.9570        %    ice cover (fraction of grid box)
       sit       0.0000       0.0342       7.8664        m    ice thickness
       tas     -45.6267      12.0780      31.4151        C    2 m temperature
       uas     -14.6180      -0.1182      19.8541      m/s    zonal wind in 10m
       vas     -14.5301      -0.4894      12.4823      m/s    meridional wind in 10m
   sfcwind       0.5706       7.2617      22.2255      m/s    10m Wind Speed
      hfss    -251.7140     -14.4240     420.4320     W/m2    sensible heat flux
      hfls    -377.8920     -89.2946      69.2690     W/m2    latent heat flux
      tauu   -2492.7800      17.9079    4723.6299    mN/m2    u-stress
      tauv   -2389.9900      -7.2535    2524.3301    mN/m2    v-stress
      rlus     141.8240     389.0540     518.0530     W/m2    LW up surface
  net_flux    -586.9370       7.9012     307.4920     W/m2    surface net energy flux
      rlnt    -312.1010    -237.1290    -135.3960     W/m2    net top LW radiation  (-OLR)
      rsdt       0.0000     350.5400     486.9830     W/m2    top incoming SW radiation