table_ngc4008_HP9_2033-JJA.txt Thu Mar 07 07:18:54 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       psl     949.1770    1000.9100    1020.4800      hPa    mean sea level pressure
       prw       0.0962      22.9796      60.9058    kg/m2    vertically integrated water vapor
     cllvi       0.0000      92.2772    1125.9301     g/m2    vertically integrated cloud water
     clivi       0.0000       9.6047     114.9660     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0142       1.0199    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0151       0.3463    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0530       0.9607    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.2763     145.8800     mm/d    total precipitation
      prls       0.0000       0.2090      67.2308     mm/d    precip large scale snow
      rsdt       0.0000     330.3610     459.6310     W/m2    top incoming SW radiation(down)
      rsds       0.0000     181.7300     369.2420     W/m2    SW surface(down)
      rsus       0.0000      22.0324     271.5030     W/m2    SW surface(up)
      rsut       0.0000      92.7372     280.6580     W/m2    TOA Outgoing SW Radiation(up)
      rsnt       0.0000     237.6240     407.2940     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       0.0000     159.6970     325.1630     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      58.7437     352.0380     459.1790     W/m2    LW down surface(down)
      rlus      78.9942     408.2780     602.2980     W/m2    LW up surface(up)
      rlus      78.9942     408.2780     602.2980     W/m2    olr(up)
      rlns     -19.8904      56.2402     187.9260     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -186.8500      -5.5885     156.3170     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -385.7350    -248.5810     -47.6206     W/m2    rsns-rlns(down)
        ts     -80.1617      17.1282      46.8561        C    surface temperature
       sic       0.0000       3.2143      99.9738        %    ice cover (fraction of grid box)
       sit       0.0000       0.0314       6.9053        m    ice thickness
       tas     -72.9262      15.8791      42.8420        C    2 m temperature
       uas     -15.8819       0.1216      14.6692      m/s    zonal wind in 10m
       vas     -13.4366       0.6542      16.2739      m/s    meridional wind in 10m
   sfcwind       0.8410       7.1724      18.3681      m/s    10m Wind Speed
      hfss    -206.0410     -21.0752     226.7210     W/m2    sensible heat flux
      hfls    -322.1620     -89.6937     150.5810     W/m2    latent heat flux
      tauu   -1788.7300      15.7139    3169.1399    mN/m2    u-stress
      tauv   -1736.5000       7.5946    2265.4900    mN/m2    v-stress
      rlus      78.9942     408.2780     602.2980     W/m2    LW up surface
  net_flux    -398.4730      -7.3117     356.5440     W/m2    surface net energy flux
      rlnt    -332.6740    -243.2130     -87.9286     W/m2    net top LW radiation  (-OLR)
      rsdt       0.0000     330.3610     459.6310     W/m2    top incoming SW radiation