table_ngc4008_HP9_2033-MAM.txt Thu Mar 07 06:40:57 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       psl     954.3830    1001.2600    1021.8800      hPa    mean sea level pressure
       prw       0.1444      20.9306      48.0329    kg/m2    vertically integrated water vapor
     cllvi       0.0000      85.3957     799.7690     g/m2    vertically integrated cloud water
     clivi       0.0003      10.2936      74.9920     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0139       0.6169    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0144       0.3305    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0531       0.9686    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.2321     124.6650     mm/d    total precipitation
      prls       0.0000       0.2858      48.5474     mm/d    precip large scale snow
      rsdt      21.2191     338.3370     433.3520     W/m2    top incoming SW radiation(down)
      rsds      11.2045     192.7170     338.8520     W/m2    SW surface(down)
      rsus       1.1815      26.3591     270.8320     W/m2    SW surface(up)
      rsut      13.4604      95.9405     264.2290     W/m2    TOA Outgoing SW Radiation(up)
      rsnt       6.8051     242.3970     384.9610     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       2.2042     166.3580     299.5790     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      67.0128     341.9990     433.0940     W/m2    LW down surface(down)
      rlus      95.2182     399.0910     521.4750     W/m2    LW up surface(up)
      rlus      95.2182     399.0910     521.4750     W/m2    olr(up)
      rlns      -0.9458      57.0928     151.7880     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -170.1860       2.7670     140.5580     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -337.0050    -232.7340       6.7063     W/m2    rsns-rlns(down)
        ts     -71.1099      15.3879      36.3575        C    surface temperature
       sic       0.0000       2.9587      99.9939        %    ice cover (fraction of grid box)
       sit       0.0000       0.0455       9.7462        m    ice thickness
       tas     -65.4854      14.0810      35.0005        C    2 m temperature
       uas     -13.9726      -0.1122      15.7781      m/s    zonal wind in 10m
       vas     -12.0779      -0.0349      14.4061      m/s    meridional wind in 10m
   sfcwind       1.1125       7.1079      18.4579      m/s    10m Wind Speed
      hfss    -188.3450     -19.5361     204.6650     W/m2    sensible heat flux
      hfls    -279.4500     -88.0767      30.9063     W/m2    latent heat flux
      tauu   -1910.5000      14.1013    4201.6602    mN/m2    u-stress
      tauv   -1914.9700       0.9036    1448.0000    mN/m2    v-stress
      rlus      95.2182     399.0910     521.4750     W/m2    LW up surface
  net_flux    -414.2660       1.6522     309.6730     W/m2    surface net energy flux
      rlnt    -323.8010    -239.6300    -106.6320     W/m2    net top LW radiation  (-OLR)
      rsdt      21.2191     338.3370     433.3520     W/m2    top incoming SW radiation