table_ngc4008_HP9_2033-SON.txt Thu Mar 07 07:41:49 2024 1

---------------------------------------------------------------------------------------------------
      name          min      fldmean          max     unit    description
---------------------------------------------------------------------------------------------------
       psl     951.3830    1001.2200    1020.5400      hPa    mean sea level pressure
       prw       0.1049      21.6356      49.1909    kg/m2    vertically integrated water vapor
     cllvi       0.0000      87.2199     801.5490     g/m2    vertically integrated cloud water
     clivi       0.0000      10.1432      78.3839     g/m2    vertically integrated cloud ice
      qgvi       0.0000       0.0136       0.9186    kg/m2    total_graupel vertically integrated graupel
      qrvi       0.0000       0.0147       0.4070    kg/m2    total_rain  vertically integrated r
      qsvi       0.0000       0.0526       0.8949    kg/m2    total_snow  vertically integrated s
        pr       0.0000       3.2491     149.6620     mm/d    total precipitation
      prls       0.0000       0.2697      72.5505     mm/d    precip large scale snow
      rsdt      25.3519     341.9790     436.9260     W/m2    top incoming SW radiation(down)
      rsds       6.2638     192.4240     386.5390     W/m2    SW surface(down)
      rsus       0.4459      26.7962     255.5300     W/m2    SW surface(up)
      rsut      10.7933      99.3761     274.3850     W/m2    TOA Outgoing SW Radiation(up)
      rsnt      10.3418     242.6030     387.5530     W/m2    TOA net SW flux (rsdt-rsut)(down)
      rsns       2.8837     165.6280     329.4040     W/m2    Surface net SW flux ( rsds-rsus) (do
      rlds      62.1487     343.7950     430.8590     W/m2    LW down surface(down)
      rlus      98.2410     399.6660     530.2850     W/m2    LW up surface(up)
      rlus      98.2410     399.6660     530.2850     W/m2    olr(up)
      rlns       3.0919      55.8705     177.7430     W/m2    Surface net LW flux (rlus-rlds) (u
      rtnt    -181.1990       2.4493     146.0390     W/m2    TOA net energy flux (rsnt-rlut)(do
      rtns    -352.9380    -234.0380      40.3407     W/m2    rsns-rlns(down)
        ts     -70.1325      15.5593      37.1696        C    surface temperature
       sic       0.0000       3.4422      99.8793        %    ice cover (fraction of grid box)
       sit       0.0000       0.0348       8.0547        m    ice thickness
       tas     -64.6838      14.2401      33.0300        C    2 m temperature
       uas     -14.1847      -0.0470      17.6094      m/s    zonal wind in 10m
       vas     -14.6290       0.2618      13.5667      m/s    meridional wind in 10m
   sfcwind       0.9692       7.1785      20.5415      m/s    10m Wind Speed
      hfss    -200.7140     -16.9594     236.2670     W/m2    sensible heat flux
      hfls    -304.9230     -87.1802      84.3978     W/m2    latent heat flux
      tauu   -1484.8101      16.2430    4304.7700    mN/m2    u-stress
      tauv   -2197.1201       0.8440    1352.8199    mN/m2    v-stress
      rlus      98.2410     399.6660     530.2850     W/m2    LW up surface
  net_flux    -357.9240       5.6180     215.8490     W/m2    surface net energy flux
      rlnt    -314.8460    -240.1540    -103.6610     W/m2    net top LW radiation  (-OLR)
      rsdt      25.3519     341.9790     436.9260     W/m2    top incoming SW radiation